**1 x DM32 WiFi Digital Gauge Package**

* DM32 WiFi Dual Channel Color Touchscreen Manometer
* USB Cable, 6' (1.8 m)
* Cat5 Cable, 7' (2 m) Blue
* DM32 USB Charging Module (120V/60Hz, 240V/50Hz, or 110V/50Hz)
* Gauge Case
* DM32 Magnetic Clip
* ISO17025 calibration of DM32
* Gauge Calibration Verification Report

**1 x 5000 Series Fan Set**

* 5000 Series Calibrated Fan (120V/60Hz, 240V/50Hz, or 110V/50Hz)
* Range Ring A for 5000/6000 Series Fan
* B8 Plate for 5000/6000 Series Fan
* 8 x 4" Blank Plugs
* Ranges 74,47 and 29
* Power Cord
* 1 x Fan Cover
* System Calibration Verification Report

**1 x Regular Cloth Door Panel & Frame (new) - Single Fan**

* Aluminum Frame, Red Anodized
* Cloth for 1000/2000/3000/5000/6000 Series Fan, Regular Height
* Fan Crossbar Strap for Aluminum Frame
* Case for Aluminum Frame
* *\*\*Optional: 50" Large Aluminum Frame Offered At Additional Cost\*\**

**1 x Case for System Accessories**

**1 x Fan Case**

**4 x Roll of Grill Masks**

**1 x Blower Door Tubing Kit**

**1 x Umbilical for 1000/5000/6000 Series Fan, 7 ft (2 m)**

|  |
| --- |
| **Specifications below are for each individual fan.** |
| Fan Model #: | 5000 |  |
|   | Flow Into: | CFM | litres/sec | m3/h |  |
|  Maximum Flow, per fan (60 Hz) reduce values by 15% for 50Hz fan | Free Air | 6,400 | 3,020 | 10,874 |  |
| **50 Pa** | 5,700 | 2,690 | 9,684 |  |
| **75 Pa** | 5,400 | 2,549 | 9,175 |  |
| Minimum Flow:-on Range B29 |  **50 Pa** | 9 | 4 | 15 |  |
| Dimensions: | 22" (55.9 cm) inlet diameter, 9.75" (24.8 cm) long, 25" (63.5 cm) height |  |
| Weight: | 33.5 lb (15.2 kg) or 35.2 lb (16.0 kg) with Ring A & Plated B8 installed |  |
| Flow Accuracy: | +/-5% |  |
| Power: | 120V@60hz/11A or 240V@50hz/4.9A or 110V@50Hz/ 8.9A |  |
| Recommended Fan Calibration Interval: | 5 years |  |