**1 x DM32 WiFi Digital Gauge Package**

* DM32 WiFi Dual Channel Color Touchscreen Manometer
* USB Cable, 6' (1.8 m)
* Cat5 Cable, 7' (2 m) Blue
* DM32 USB Charging Module (120V/60Hz, 240V/50Hz, or 110V/50Hz)
* Gauge Case
* DM32 Magnetic Clip
* ISO17025 calibration of DM32
* Gauge Calibration Verification Report

**1 x 6000 Series Fan Set**

* 6000 Series Calibrated Fan (120V/60Hz, 240V/50Hz, or 110V/50Hz)
* Range Ring A for 5000/6000 Series Fan
* B8 Plate for 5000/6000 Series Fan
* 1 x High Power Drive for 6000 Series Fan (120V/60Hz, 240V/50Hz, or 110V/50Hz)
* Range 74,47, 29
* 8 x 4" Blank Plugs
* Power Cord
* 2 x Fan Cover
* System Calibration Verification Report

**1 x Hard Panel Set for 1000/5000/6000 Series Fan**

**1 x Blower Door Tubing Kit**

**4 x Roll of Grill Masks**

**1 x Umbilical for 1000/5000/6000 Series Fan, 7 ft (2 m)**

**1 x Large Frame Package**

**1 x Fan Case**

**1 x Accessory Case**



|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Specifications below are for each individual fan.** | | | | |
| Fan Model #: | 6000 | | | |  |
|  | Flow Into: | CFM | litres/sec | m3/h |  |
| Maximum Flow\*, per fan | Free Air | 8,100 | 3,823 | 13,762 |  |
| **50 Pa** | 7,700 | 3,634 | 13,082 |  |
| **75 Pa** | 7,400 | 3,492 | 12,573 |  |
| Minimum Flow:  on Range 29 | **50 Pa** | 9 | 4 | 15 |  |
| Dimensions: | 26" × 25.5" × 9.5" (66 x 65 x 24 cm) | | | |  |
| Weight: | 36.3 lb (16.5 kg) or 38 lb (17.2 kg) with Ring A & Plated B8 installed | | | |  |
| Flow Accuracy: | +/-5% | | | |  |
| Power: | 120V@60hz/22.0A or 240V@50hz/10.9A or 110V@50Hz/22.0A | | | |  |
| Recommended Fan Calibration Interval: | 5 years | | | |  |

